**Quick Guide**

Graphical user interface

Description automatically generated with medium confidence

5

4

3

2

1

Line 2

Line 1

1. Select Marking Line 1 or Line 2.
2. Adjust Marking Position.
3. Adjust Marking Character Size.
4. Adjust Marking Clarity
5. Save changes.

Steps:

1. Identify which line to adjust. Then select[1] the proper **line no**.
2. Marking clarity is affected by the combination[4] of **Current**, **QSW** and the **Speed**.
3. With refer to the marking layout below. To adjust the position Up/Down, change the data of X-Axis data. The higher the value will move the marking position in upper direction. The lower the value will move the marking position downwards. To adjust the position left/right, change the data of Y-Axis. The higher the value will move the position to the right. The lower the value will move the marking towards left side.

A picture containing graphical user interface

Description automatically generated

1. Note, every changes you have done. It is advisable to save[5] the changes before switch to another line. You can post the data once you have saved. The data is save to the database.